A B C D E F G H I L M N O P R S T U V W

## F

FastSerial - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  Hardware Option - Fast Serial
FIFO - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  Hardware Option - 245 FIFO
FIFOTarget - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  Hardware Option - 245 FIFO CPU Target
flags - Variable in class com.ftdi.j2xx.D2xxManager.FtDeviceInfoListNode
  Indicates if device is already open (`D2xxManager.FT_FLAGS_OPENED`), or supports hi-speed (`D2xxManager.FT_FLAGS_HI_SPEED`).
FT1248 - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  Hardware Option - FT1248
FT1248ClockPolarity - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  FT1248 Option - FT1248 clock polarity, true = clock idle high, false = clock idle low
FT1248ClockPolarity - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  FT1248 Option - FT1248 clock polarity, true = clock idle high, false = clock idle low
FT1248FlowControl - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  FT1248 Option - FT1248 Flow Control
FT1248FlowControl - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  FT1248 Option - FT1248 Flow Control
FT1248LSB - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  FT1248 Option - FT1248 LSB, true = LSB, false = MSB
FT1248LSB - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  FT1248 Option - FT1248 LSB, true = LSB, false = MSB
FT4222_CLK_NOT_SUPPORTED - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_DEVICE_LIST_NOT_READY - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_DEVICE_NOT_FOUND - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_DEVICE_NOT_OPENED - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_DEVICE_NOT_OPENED_FOR_ERASE - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_DEVICE_NOT_OPENED_FOR_WRITE - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_DEVICE_NOT_SUPPORTED - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_EEPROM_ERASE_FAILED - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_EEPROM_NOT_PRESENT - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_EEPROM_NOT_PROGRAMMED - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_EEPROM_READ_FAILED - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_EEPROM_WRITE_FAILED - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_EVENT_NOT_SUPPORTED - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_EXCEED_ARRAY_LENGTH - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_EXCEEDED_MAX_TRANSFER_SIZE - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_FAILED_TO_READ_DEVICE - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_FAILED_TO_WRITE_DEVICE - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_FUN_NOT_SUPPORT - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_GPIO_EXCEEDED_MAX_PORTNUM - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_GPIO_INPUT_NOT_SUPPORTED - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_GPIO_NOT_SUPPORTED_IN_THIS_MODE - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_GPIO_OPENDRAIN_INVALID_IN_OUTPUTMODE - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_GPIO_PULLDOWN_INVALID_IN_INPUTMODE - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_GPIO_PULLUP_INVALID_IN_INPUTMODE - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_GPIO_WRITE_NOT_SUPPORTED - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_I2C_MASTER - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_FUNCTION
FT4222_I2C_NOT_SUPPORTED_IN_THIS_MODE - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_I2C_SLAVE - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_FUNCTION
FT4222_INSUFFICIENT_RESOURCES - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_INTERRUPT_NOT_SUPPORTED - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_INVAILD_FUNCTION - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_INVALID_ARGS - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_INVALID_BAUD_RATE - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_INVALID_HANDLE - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_INVALID_PARAMETER - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_INVALID_POINTER - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_IO_ERROR - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_IS_NOT_I2C_MODE - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_IS_NOT_SPI_MODE - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_IS_NOT_SPI_MULTI_MODE - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_IS_NOT_SPI_SINGLE_MODE - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_NOT_SUPPORTED - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_OK - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_OTHER_ERROR - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_SPI_MASTER - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_FUNCTION
FT4222_SPI_SLAVE - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_FUNCTION
FT4222_SPI_SLAVE_SYNC_WORD - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.SPI_SLAVE_CMD
FT4222_VENDER_CMD_NOT_SUPPORTED - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT4222_WRONG_I2C_ADDR - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT_4222_Defines - Class in com.ftdi.j2xx.ft4222
FT_4222_Defines() - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_Defines
FT_4222_Defines.CHIPTOP_CMD - Class in com.ftdi.j2xx.ft4222
FT_4222_Defines.CHIPTOP_CMD() - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
FT_4222_Defines.FT4222_ClockRate - Class in com.ftdi.j2xx.ft4222
FT_4222_Defines.FT4222_ClockRate() - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_ClockRate
FT_4222_Defines.FT4222_FUNCTION - Class in com.ftdi.j2xx.ft4222
FT_4222_Defines.FT4222_FUNCTION() - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_FUNCTION
FT_4222_Defines.FT4222_SPIClock - Class in com.ftdi.j2xx.ft4222
FT_4222_Defines.FT4222_SPIClock() - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_SPIClock
FT_4222_Defines.FT4222_SPICPHA - Class in com.ftdi.j2xx.ft4222
FT_4222_Defines.FT4222_SPICPHA() - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_SPICPHA
FT_4222_Defines.FT4222_SPICPOL - Class in com.ftdi.j2xx.ft4222
FT_4222_Defines.FT4222_SPICPOL() - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_SPICPOL
FT_4222_Defines.FT4222_SPIMode - Class in com.ftdi.j2xx.ft4222
FT_4222_Defines.FT4222_SPIMode() - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_SPIMode
FT_4222_Defines.FT4222_STATUS - Class in com.ftdi.j2xx.ft4222
FT_4222_Defines.FT4222_STATUS() - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_STATUS
FT_4222_Defines.GPIO_Dir - Class in com.ftdi.j2xx.ft4222
FT_4222_Defines.GPIO_Dir() - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_Defines.GPIO_Dir
FT_4222_Defines.GPIO_Output - Class in com.ftdi.j2xx.ft4222
FT_4222_Defines.GPIO_Output() - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_Defines.GPIO_Output
FT_4222_Defines.GPIO_Port - Class in com.ftdi.j2xx.ft4222
FT_4222_Defines.GPIO_Port() - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_Defines.GPIO_Port
FT_4222_Defines.GPIO_Tigger - Class in com.ftdi.j2xx.ft4222
FT_4222_Defines.GPIO_Tigger() - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_Defines.GPIO_Tigger
FT_4222_Defines.I2C_CMD - Class in com.ftdi.j2xx.ft4222
FT_4222_Defines.I2C_CMD() - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_Defines.I2C_CMD
FT_4222_Defines.I2C_MasterFlag - Class in com.ftdi.j2xx.ft4222
FT_4222_Defines.I2C_MasterFlag() - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_Defines.I2C_MasterFlag
FT_4222_Defines.SPI_CMD - Class in com.ftdi.j2xx.ft4222
FT_4222_Defines.SPI_CMD() - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_Defines.SPI_CMD
FT_4222_Defines.SPI_DrivingStrength - Class in com.ftdi.j2xx.ft4222
FT_4222_Defines.SPI_DrivingStrength() - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_Defines.SPI_DrivingStrength
FT_4222_Defines.SPI_SLAVE_CMD - Class in com.ftdi.j2xx.ft4222
FT_4222_Defines.SPI_SLAVE_CMD() - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_Defines.SPI_SLAVE_CMD
FT_4222_Defines.SPI_SS - Class in com.ftdi.j2xx.ft4222
FT_4222_Defines.SPI_SS() - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_Defines.SPI_SS
FT_4222_Device - Class in com.ftdi.j2xx.ft4222
FT_4222_Device(FT_Device) - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_Device
  Constructor for FT4222 device class
FT_4222_Gpio - Class in com.ftdi.j2xx.ft4222
FT_4222_Gpio(FT_4222_Device) - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_Gpio
FT_4222_I2c_Master - Class in com.ftdi.j2xx.ft4222
FT_4222_I2c_Master(FT_4222_Device) - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_I2c_Master
FT_4222_I2c_Slave - Class in com.ftdi.j2xx.ft4222
FT_4222_I2c_Slave(FT_4222_Device) - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_I2c_Slave
FT_4222_Spi_Master - Class in com.ftdi.j2xx.ft4222
  FDI SPI master support library
FT_4222_Spi_Master(FT_4222_Device) - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_Spi_Master
FT_4222_Spi_Slave - Class in com.ftdi.j2xx.ft4222
FT_4222_Spi_Slave(FT_4222_Device) - Constructor for class com.ftdi.j2xx.ft4222.FT_4222_Spi_Slave
FT_BI - Static variable in class com.ftdi.j2xx.D2xxManager
  Line status bits :
  OE: `D2xxManager.FT_OE`,
  PE: `D2xxManager.FT_PE`,
  FE: `D2xxManager.FT_FE`,
  BI: `D2xxManager.FT_BI`
FT_BITMODE_ASYNC_BITBANG - Static variable in class com.ftdi.j2xx.D2xxManager
  Bit Mode bits :
  Reset: `D2xxManager.FT_BITMODE_RESET`,
  Asynchronous Bit Bang (FT232B, FT2232, FT232H, FT2232H, FT4232H): `D2xxManager.FT_BITMODE_ASYNC_BITBANG`,
  MPSSE (FT2232, FT2232H, FT4232H and FT232H devices only) : `D2xxManager.FT_BITMODE_MPSSE`,
  Synchronous Bit Bang (FT232R, FT245R, FT2232, FT2232H, FT4232H and FT232H devices only) : `D2xxManager.FT_BITMODE_SYNC_BITBANG`,
  MCU Host Bus Emulation Mode (FT2232, FT2232H, and FT232H devices only) : `D2xxManager.FT_BITMODE_MCU_HOST`,
  Fast Opto-Isolated Serial Mode (FT2232, FT2232H, and FT232H devices only) : `D2xxManager.FT_BITMODE_FAST_SERIAL`,
  CBUS Bit Bang Mode (FT232R and FT232H devices only) : `D2xxManager.FT_BITMODE_CBUS_BITBANG`,
  Single Channel Synchronous 245 FIFO Mode (FT2232H and FT232H devices only) : `D2xxManager.FT_BITMODE_SYNC_FIFO`
FT_BITMODE_CBUS_BITBANG - Static variable in class com.ftdi.j2xx.D2xxManager
  Bit Mode bits :
  Reset: `D2xxManager.FT_BITMODE_RESET`,
  Asynchronous Bit Bang (FT232B, FT2232, FT232H, FT2232H, FT4232H): `D2xxManager.FT_BITMODE_ASYNC_BITBANG`,
  MPSSE (FT2232, FT2232H, FT4232H and FT232H devices only) : `D2xxManager.FT_BITMODE_MPSSE`,
  Synchronous Bit Bang (FT232R, FT245R, FT2232, FT2232H, FT4232H and FT232H devices only) : `D2xxManager.FT_BITMODE_SYNC_BITBANG`,
  MCU Host Bus Emulation Mode (FT2232, FT2232H, and FT232H devices only) : `D2xxManager.FT_BITMODE_MCU_HOST`,
  Fast Opto-Isolated Serial Mode (FT2232, FT2232H, and FT232H devices only) : `D2xxManager.FT_BITMODE_FAST_SERIAL`,
  CBUS Bit Bang Mode (FT232R and FT232H devices only) : `D2xxManager.FT_BITMODE_CBUS_BITBANG`,
  Single Channel Synchronous 245 FIFO Mode (FT2232H and FT232H devices only) : `D2xxManager.FT_BITMODE_SYNC_FIFO`
FT_BITMODE_FAST_SERIAL - Static variable in class com.ftdi.j2xx.D2xxManager
  Bit Mode bits :
  Reset: `D2xxManager.FT_BITMODE_RESET`,
  Asynchronous Bit Bang (FT232B, FT2232, FT232H, FT2232H, FT4232H): `D2xxManager.FT_BITMODE_ASYNC_BITBANG`,
  MPSSE (FT2232, FT2232H, FT4232H and FT232H devices only) : `D2xxManager.FT_BITMODE_MPSSE`,
  Synchronous Bit Bang (FT232R, FT245R, FT2232, FT2232H, FT4232H and FT232H devices only) : `D2xxManager.FT_BITMODE_SYNC_BITBANG`,
  MCU Host Bus Emulation Mode (FT2232, FT2232H, and FT232H devices only) : `D2xxManager.FT_BITMODE_MCU_HOST`,
  Fast Opto-Isolated Serial Mode (FT2232, FT2232H, and FT232H devices only) : `D2xxManager.FT_BITMODE_FAST_SERIAL`,
  CBUS Bit Bang Mode (FT232R and FT232H devices only) : `D2xxManager.FT_BITMODE_CBUS_BITBANG`,
  Single Channel Synchronous 245 FIFO Mode (FT2232H and FT232H devices only) : `D2xxManager.FT_BITMODE_SYNC_FIFO`
FT_BITMODE_MCU_HOST - Static variable in class com.ftdi.j2xx.D2xxManager
  Bit Mode bits :
  Reset: `D2xxManager.FT_BITMODE_RESET`,
  Asynchronous Bit Bang (FT232B, FT2232, FT232H, FT2232H, FT4232H): `D2xxManager.FT_BITMODE_ASYNC_BITBANG`,
  MPSSE (FT2232, FT2232H, FT4232H and FT232H devices only) : `D2xxManager.FT_BITMODE_MPSSE`,
  Synchronous Bit Bang (FT232R, FT245R, FT2232, FT2232H, FT4232H and FT232H devices only) : `D2xxManager.FT_BITMODE_SYNC_BITBANG`,
  MCU Host Bus Emulation Mode (FT2232, FT2232H, and FT232H devices only) : `D2xxManager.FT_BITMODE_MCU_HOST`,
  Fast Opto-Isolated Serial Mode (FT2232, FT2232H, and FT232H devices only) : `D2xxManager.FT_BITMODE_FAST_SERIAL`,
  CBUS Bit Bang Mode (FT232R and FT232H devices only) : `D2xxManager.FT_BITMODE_CBUS_BITBANG`,
  Single Channel Synchronous 245 FIFO Mode (FT2232H and FT232H devices only) : `D2xxManager.FT_BITMODE_SYNC_FIFO`
FT_BITMODE_MPSSE - Static variable in class com.ftdi.j2xx.D2xxManager
  Bit Mode bits :
  Reset: `D2xxManager.FT_BITMODE_RESET`,
  Asynchronous Bit Bang (FT232B, FT2232, FT232H, FT2232H, FT4232H): `D2xxManager.FT_BITMODE_ASYNC_BITBANG`,
  MPSSE (FT2232, FT2232H, FT4232H and FT232H devices only) : `D2xxManager.FT_BITMODE_MPSSE`,
  Synchronous Bit Bang (FT232R, FT245R, FT2232, FT2232H, FT4232H and FT232H devices only) : `D2xxManager.FT_BITMODE_SYNC_BITBANG`,
  MCU Host Bus Emulation Mode (FT2232, FT2232H, and FT232H devices only) : `D2xxManager.FT_BITMODE_MCU_HOST`,
  Fast Opto-Isolated Serial Mode (FT2232, FT2232H, and FT232H devices only) : `D2xxManager.FT_BITMODE_FAST_SERIAL`,
  CBUS Bit Bang Mode (FT232R and FT232H devices only) : `D2xxManager.FT_BITMODE_CBUS_BITBANG`,
  Single Channel Synchronous 245 FIFO Mode (FT2232H and FT232H devices only) : `D2xxManager.FT_BITMODE_SYNC_FIFO`
FT_BITMODE_RESET - Static variable in class com.ftdi.j2xx.D2xxManager
  Bit Mode bits :
  Reset: `D2xxManager.FT_BITMODE_RESET`,
  Asynchronous Bit Bang (FT232B, FT2232, FT232H, FT2232H, FT4232H): `D2xxManager.FT_BITMODE_ASYNC_BITBANG`,
  MPSSE (FT2232, FT2232H, FT4232H and FT232H devices only) : `D2xxManager.FT_BITMODE_MPSSE`,
  Synchronous Bit Bang (FT232R, FT245R, FT2232, FT2232H, FT4232H and FT232H devices only) : `D2xxManager.FT_BITMODE_SYNC_BITBANG`,
  MCU Host Bus Emulation Mode (FT2232, FT2232H, and FT232H devices only) : `D2xxManager.FT_BITMODE_MCU_HOST`,
  Fast Opto-Isolated Serial Mode (FT2232, FT2232H, and FT232H devices only) : `D2xxManager.FT_BITMODE_FAST_SERIAL`,
  CBUS Bit Bang Mode (FT232R and FT232H devices only) : `D2xxManager.FT_BITMODE_CBUS_BITBANG`,
  Single Channel Synchronous 245 FIFO Mode (FT2232H and FT232H devices only) : `D2xxManager.FT_BITMODE_SYNC_FIFO`
FT_BITMODE_SYNC_BITBANG - Static variable in class com.ftdi.j2xx.D2xxManager
  Bit Mode bits :
  Reset: `D2xxManager.FT_BITMODE_RESET`,
  Asynchronous Bit Bang (FT232B, FT2232, FT232H, FT2232H, FT4232H): `D2xxManager.FT_BITMODE_ASYNC_BITBANG`,
  MPSSE (FT2232, FT2232H, FT4232H and FT232H devices only) : `D2xxManager.FT_BITMODE_MPSSE`,
  Synchronous Bit Bang (FT232R, FT245R, FT2232, FT2232H, FT4232H and FT232H devices only) : `D2xxManager.FT_BITMODE_SYNC_BITBANG`,
  MCU Host Bus Emulation Mode (FT2232, FT2232H, and FT232H devices only) : `D2xxManager.FT_BITMODE_MCU_HOST`,
  Fast Opto-Isolated Serial Mode (FT2232, FT2232H, and FT232H devices only) : `D2xxManager.FT_BITMODE_FAST_SERIAL`,
  CBUS Bit Bang Mode (FT232R and FT232H devices only) : `D2xxManager.FT_BITMODE_CBUS_BITBANG`,
  Single Channel Synchronous 245 FIFO Mode (FT2232H and FT232H devices only) : `D2xxManager.FT_BITMODE_SYNC_FIFO`
FT_BITMODE_SYNC_FIFO - Static variable in class com.ftdi.j2xx.D2xxManager
  Bit Mode bits :
  Reset: `D2xxManager.FT_BITMODE_RESET`,
  Asynchronous Bit Bang (FT232B, FT2232, FT232H, FT2232H, FT4232H): `D2xxManager.FT_BITMODE_ASYNC_BITBANG`,
  MPSSE (FT2232, FT2232H, FT4232H and FT232H devices only) : `D2xxManager.FT_BITMODE_MPSSE`,
  Synchronous Bit Bang (FT232R, FT245R, FT2232, FT2232H, FT4232H and FT232H devices only) : `D2xxManager.FT_BITMODE_SYNC_BITBANG`,
  MCU Host Bus Emulation Mode (FT2232, FT2232H, and FT232H devices only) : `D2xxManager.FT_BITMODE_MCU_HOST`,
  Fast Opto-Isolated Serial Mode (FT2232, FT2232H, and FT232H devices only) : `D2xxManager.FT_BITMODE_FAST_SERIAL`,
  CBUS Bit Bang Mode (FT232R and FT232H devices only) : `D2xxManager.FT_BITMODE_CBUS_BITBANG`,
  Single Channel Synchronous 245 FIFO Mode (FT2232H and FT232H devices only) : `D2xxManager.FT_BITMODE_SYNC_FIFO`
FT_CTS - Static variable in class com.ftdi.j2xx.D2xxManager
  Modem status bits :
  CTS: `D2xxManager.FT_CTS`,
  DSR: `D2xxManager.FT_DSR`,
  RI: `D2xxManager.FT_RI`,
  DCD: `D2xxManager.FT_DCD`
FT_DATA_BITS_7 - Static variable in class com.ftdi.j2xx.D2xxManager
  Data bits :
  7 : `D2xxManager.FT_DATA_BITS_7`,
  8 : `D2xxManager.FT_DATA_BITS_8`
FT_DATA_BITS_8 - Static variable in class com.ftdi.j2xx.D2xxManager
  Data bits :
  7 : `D2xxManager.FT_DATA_BITS_7`,
  8 : `D2xxManager.FT_DATA_BITS_8`
FT_DCD - Static variable in class com.ftdi.j2xx.D2xxManager
  Modem status bits :
  CTS: `D2xxManager.FT_CTS`,
  DSR: `D2xxManager.FT_DSR`,
  RI: `D2xxManager.FT_RI`,
  DCD: `D2xxManager.FT_DCD`
FT_Device - Class in com.ftdi.j2xx
  A device class provide different APIs for host to communicate and operate different FT device.
FT_Device(Context, UsbManager, UsbDevice, UsbInterface) - Constructor for class com.ftdi.j2xx.FT_Device
  FT_Device constructor
FT_DEVICE_2232 - Static variable in class com.ftdi.j2xx.D2xxManager
  Device Type :
  bvdDevice = 0x0200 or 0x0400 and iSerialNumber != 0: `D2xxManager.FT_DEVICE_232B`,
  bvdDevice = 0x0200 and iSerialNumber != 0 : `D2xxManager.FT_DEVICE_8U232AM`,
  Unknown : `D2xxManager.FT_DEVICE_UNKNOWN`,
  bvdDevice = 0x0500 : `D2xxManager.FT_DEVICE_2232`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_232R`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_245R`,
  bvdDevice = 0x0700 : `D2xxManager.FT_DEVICE_2232H`,
  bvdDevice = 0x0800 : `D2xxManager.FT_DEVICE_4232H`,
  bvdDevice = 0x0900 : `D2xxManager.FT_DEVICE_232H`,
  bvdDevice = 0x1000 : `D2xxManager.FT_DEVICE_X_SERIES`
  bvdDevice = 0x1800 : `#FT_DEVICE_4222`
  bvdDevice = 0x1900 : `#FT_DEVICE_4222`
  bvdDevice = 0x1700 : `#FT_DEVICE_4222`
FT_DEVICE_2232H - Static variable in class com.ftdi.j2xx.D2xxManager
  Device Type :
  bvdDevice = 0x0200 or 0x0400 and iSerialNumber != 0: `D2xxManager.FT_DEVICE_232B`,
  bvdDevice = 0x0200 and iSerialNumber != 0 : `D2xxManager.FT_DEVICE_8U232AM`,
  Unknown : `D2xxManager.FT_DEVICE_UNKNOWN`,
  bvdDevice = 0x0500 : `D2xxManager.FT_DEVICE_2232`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_232R`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_245R`,
  bvdDevice = 0x0700 : `D2xxManager.FT_DEVICE_2232H`,
  bvdDevice = 0x0800 : `D2xxManager.FT_DEVICE_4232H`,
  bvdDevice = 0x0900 : `D2xxManager.FT_DEVICE_232H`,
  bvdDevice = 0x1000 : `D2xxManager.FT_DEVICE_X_SERIES`
  bvdDevice = 0x1800 : `#FT_DEVICE_4222`
  bvdDevice = 0x1900 : `#FT_DEVICE_4222`
  bvdDevice = 0x1700 : `#FT_DEVICE_4222`
FT_DEVICE_232B - Static variable in class com.ftdi.j2xx.D2xxManager
  Device Type :
  bvdDevice = 0x0200 or 0x0400 and iSerialNumber != 0: `D2xxManager.FT_DEVICE_232B`,
  bvdDevice = 0x0200 and iSerialNumber != 0 : `D2xxManager.FT_DEVICE_8U232AM`,
  Unknown : `D2xxManager.FT_DEVICE_UNKNOWN`,
  bvdDevice = 0x0500 : `D2xxManager.FT_DEVICE_2232`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_232R`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_245R`,
  bvdDevice = 0x0700 : `D2xxManager.FT_DEVICE_2232H`,
  bvdDevice = 0x0800 : `D2xxManager.FT_DEVICE_4232H`,
  bvdDevice = 0x0900 : `D2xxManager.FT_DEVICE_232H`,
  bvdDevice = 0x1000 : `D2xxManager.FT_DEVICE_X_SERIES`
  bvdDevice = 0x1800 : `#FT_DEVICE_4222`
  bvdDevice = 0x1900 : `#FT_DEVICE_4222`
  bvdDevice = 0x1700 : `#FT_DEVICE_4222`
FT_DEVICE_232H - Static variable in class com.ftdi.j2xx.D2xxManager
  Device Type :
  bvdDevice = 0x0200 or 0x0400 and iSerialNumber != 0: `D2xxManager.FT_DEVICE_232B`,
  bvdDevice = 0x0200 and iSerialNumber != 0 : `D2xxManager.FT_DEVICE_8U232AM`,
  Unknown : `D2xxManager.FT_DEVICE_UNKNOWN`,
  bvdDevice = 0x0500 : `D2xxManager.FT_DEVICE_2232`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_232R`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_245R`,
  bvdDevice = 0x0700 : `D2xxManager.FT_DEVICE_2232H`,
  bvdDevice = 0x0800 : `D2xxManager.FT_DEVICE_4232H`,
  bvdDevice = 0x0900 : `D2xxManager.FT_DEVICE_232H`,
  bvdDevice = 0x1000 : `D2xxManager.FT_DEVICE_X_SERIES`
  bvdDevice = 0x1800 : `#FT_DEVICE_4222`
  bvdDevice = 0x1900 : `#FT_DEVICE_4222`
  bvdDevice = 0x1700 : `#FT_DEVICE_4222`
FT_DEVICE_232R - Static variable in class com.ftdi.j2xx.D2xxManager
  Device Type :
  bvdDevice = 0x0200 or 0x0400 and iSerialNumber != 0: `D2xxManager.FT_DEVICE_232B`,
  bvdDevice = 0x0200 and iSerialNumber != 0 : `D2xxManager.FT_DEVICE_8U232AM`,
  Unknown : `D2xxManager.FT_DEVICE_UNKNOWN`,
  bvdDevice = 0x0500 : `D2xxManager.FT_DEVICE_2232`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_232R`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_245R`,
  bvdDevice = 0x0700 : `D2xxManager.FT_DEVICE_2232H`,
  bvdDevice = 0x0800 : `D2xxManager.FT_DEVICE_4232H`,
  bvdDevice = 0x0900 : `D2xxManager.FT_DEVICE_232H`,
  bvdDevice = 0x1000 : `D2xxManager.FT_DEVICE_X_SERIES`
  bvdDevice = 0x1800 : `#FT_DEVICE_4222`
  bvdDevice = 0x1900 : `#FT_DEVICE_4222`
  bvdDevice = 0x1700 : `#FT_DEVICE_4222`
FT_DEVICE_245R - Static variable in class com.ftdi.j2xx.D2xxManager
  Device Type :
  bvdDevice = 0x0200 or 0x0400 and iSerialNumber != 0: `D2xxManager.FT_DEVICE_232B`,
  bvdDevice = 0x0200 and iSerialNumber != 0 : `D2xxManager.FT_DEVICE_8U232AM`,
  Unknown : `D2xxManager.FT_DEVICE_UNKNOWN`,
  bvdDevice = 0x0500 : `D2xxManager.FT_DEVICE_2232`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_232R`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_245R`,
  bvdDevice = 0x0700 : `D2xxManager.FT_DEVICE_2232H`,
  bvdDevice = 0x0800 : `D2xxManager.FT_DEVICE_4232H`,
  bvdDevice = 0x0900 : `D2xxManager.FT_DEVICE_232H`,
  bvdDevice = 0x1000 : `D2xxManager.FT_DEVICE_X_SERIES`
  bvdDevice = 0x1800 : `#FT_DEVICE_4222`
  bvdDevice = 0x1900 : `#FT_DEVICE_4222`
  bvdDevice = 0x1700 : `#FT_DEVICE_4222`
FT_DEVICE_4222_0 - Static variable in class com.ftdi.j2xx.D2xxManager
  Device Type :
  bvdDevice = 0x0200 or 0x0400 and iSerialNumber != 0: `D2xxManager.FT_DEVICE_232B`,
  bvdDevice = 0x0200 and iSerialNumber != 0 : `D2xxManager.FT_DEVICE_8U232AM`,
  Unknown : `D2xxManager.FT_DEVICE_UNKNOWN`,
  bvdDevice = 0x0500 : `D2xxManager.FT_DEVICE_2232`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_232R`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_245R`,
  bvdDevice = 0x0700 : `D2xxManager.FT_DEVICE_2232H`,
  bvdDevice = 0x0800 : `D2xxManager.FT_DEVICE_4232H`,
  bvdDevice = 0x0900 : `D2xxManager.FT_DEVICE_232H`,
  bvdDevice = 0x1000 : `D2xxManager.FT_DEVICE_X_SERIES`
  bvdDevice = 0x1800 : `#FT_DEVICE_4222`
  bvdDevice = 0x1900 : `#FT_DEVICE_4222`
  bvdDevice = 0x1700 : `#FT_DEVICE_4222`
FT_DEVICE_4222_1_2 - Static variable in class com.ftdi.j2xx.D2xxManager
  Device Type :
  bvdDevice = 0x0200 or 0x0400 and iSerialNumber != 0: `D2xxManager.FT_DEVICE_232B`,
  bvdDevice = 0x0200 and iSerialNumber != 0 : `D2xxManager.FT_DEVICE_8U232AM`,
  Unknown : `D2xxManager.FT_DEVICE_UNKNOWN`,
  bvdDevice = 0x0500 : `D2xxManager.FT_DEVICE_2232`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_232R`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_245R`,
  bvdDevice = 0x0700 : `D2xxManager.FT_DEVICE_2232H`,
  bvdDevice = 0x0800 : `D2xxManager.FT_DEVICE_4232H`,
  bvdDevice = 0x0900 : `D2xxManager.FT_DEVICE_232H`,
  bvdDevice = 0x1000 : `D2xxManager.FT_DEVICE_X_SERIES`
  bvdDevice = 0x1800 : `#FT_DEVICE_4222`
  bvdDevice = 0x1900 : `#FT_DEVICE_4222`
  bvdDevice = 0x1700 : `#FT_DEVICE_4222`
FT_DEVICE_4222_3 - Static variable in class com.ftdi.j2xx.D2xxManager
  Device Type :
  bvdDevice = 0x0200 or 0x0400 and iSerialNumber != 0: `D2xxManager.FT_DEVICE_232B`,
  bvdDevice = 0x0200 and iSerialNumber != 0 : `D2xxManager.FT_DEVICE_8U232AM`,
  Unknown : `D2xxManager.FT_DEVICE_UNKNOWN`,
  bvdDevice = 0x0500 : `D2xxManager.FT_DEVICE_2232`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_232R`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_245R`,
  bvdDevice = 0x0700 : `D2xxManager.FT_DEVICE_2232H`,
  bvdDevice = 0x0800 : `D2xxManager.FT_DEVICE_4232H`,
  bvdDevice = 0x0900 : `D2xxManager.FT_DEVICE_232H`,
  bvdDevice = 0x1000 : `D2xxManager.FT_DEVICE_X_SERIES`
  bvdDevice = 0x1800 : `#FT_DEVICE_4222`
  bvdDevice = 0x1900 : `#FT_DEVICE_4222`
  bvdDevice = 0x1700 : `#FT_DEVICE_4222`
FT_DEVICE_4232H - Static variable in class com.ftdi.j2xx.D2xxManager
  Device Type :
  bvdDevice = 0x0200 or 0x0400 and iSerialNumber != 0: `D2xxManager.FT_DEVICE_232B`,
  bvdDevice = 0x0200 and iSerialNumber != 0 : `D2xxManager.FT_DEVICE_8U232AM`,
  Unknown : `D2xxManager.FT_DEVICE_UNKNOWN`,
  bvdDevice = 0x0500 : `D2xxManager.FT_DEVICE_2232`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_232R`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_245R`,
  bvdDevice = 0x0700 : `D2xxManager.FT_DEVICE_2232H`,
  bvdDevice = 0x0800 : `D2xxManager.FT_DEVICE_4232H`,
  bvdDevice = 0x0900 : `D2xxManager.FT_DEVICE_232H`,
  bvdDevice = 0x1000 : `D2xxManager.FT_DEVICE_X_SERIES`
  bvdDevice = 0x1800 : `#FT_DEVICE_4222`
  bvdDevice = 0x1900 : `#FT_DEVICE_4222`
  bvdDevice = 0x1700 : `#FT_DEVICE_4222`
FT_DEVICE_8U232AM - Static variable in class com.ftdi.j2xx.D2xxManager
  Device Type :
  bvdDevice = 0x0200 or 0x0400 and iSerialNumber != 0: `D2xxManager.FT_DEVICE_232B`,
  bvdDevice = 0x0200 and iSerialNumber != 0 : `D2xxManager.FT_DEVICE_8U232AM`,
  Unknown : `D2xxManager.FT_DEVICE_UNKNOWN`,
  bvdDevice = 0x0500 : `D2xxManager.FT_DEVICE_2232`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_232R`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_245R`,
  bvdDevice = 0x0700 : `D2xxManager.FT_DEVICE_2232H`,
  bvdDevice = 0x0800 : `D2xxManager.FT_DEVICE_4232H`,
  bvdDevice = 0x0900 : `D2xxManager.FT_DEVICE_232H`,
  bvdDevice = 0x1000 : `D2xxManager.FT_DEVICE_X_SERIES`
  bvdDevice = 0x1800 : `#FT_DEVICE_4222`
  bvdDevice = 0x1900 : `#FT_DEVICE_4222`
  bvdDevice = 0x1700 : `#FT_DEVICE_4222`
FT_DEVICE_UNKNOWN - Static variable in class com.ftdi.j2xx.D2xxManager
  Device Type :
  bvdDevice = 0x0200 or 0x0400 and iSerialNumber != 0: `D2xxManager.FT_DEVICE_232B`,
  bvdDevice = 0x0200 and iSerialNumber != 0 : `D2xxManager.FT_DEVICE_8U232AM`,
  Unknown : `D2xxManager.FT_DEVICE_UNKNOWN`,
  bvdDevice = 0x0500 : `D2xxManager.FT_DEVICE_2232`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_232R`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_245R`,
  bvdDevice = 0x0700 : `D2xxManager.FT_DEVICE_2232H`,
  bvdDevice = 0x0800 : `D2xxManager.FT_DEVICE_4232H`,
  bvdDevice = 0x0900 : `D2xxManager.FT_DEVICE_232H`,
  bvdDevice = 0x1000 : `D2xxManager.FT_DEVICE_X_SERIES`
  bvdDevice = 0x1800 : `#FT_DEVICE_4222`
  bvdDevice = 0x1900 : `#FT_DEVICE_4222`
  bvdDevice = 0x1700 : `#FT_DEVICE_4222`
FT_DEVICE_X_SERIES - Static variable in class com.ftdi.j2xx.D2xxManager
  Device Type :
  bvdDevice = 0x0200 or 0x0400 and iSerialNumber != 0: `D2xxManager.FT_DEVICE_232B`,
  bvdDevice = 0x0200 and iSerialNumber != 0 : `D2xxManager.FT_DEVICE_8U232AM`,
  Unknown : `D2xxManager.FT_DEVICE_UNKNOWN`,
  bvdDevice = 0x0500 : `D2xxManager.FT_DEVICE_2232`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_232R`,
  bvdDevice = 0x0600 : `D2xxManager.FT_DEVICE_245R`,
  bvdDevice = 0x0700 : `D2xxManager.FT_DEVICE_2232H`,
  bvdDevice = 0x0800 : `D2xxManager.FT_DEVICE_4232H`,
  bvdDevice = 0x0900 : `D2xxManager.FT_DEVICE_232H`,
  bvdDevice = 0x1000 : `D2xxManager.FT_DEVICE_X_SERIES`
  bvdDevice = 0x1800 : `#FT_DEVICE_4222`
  bvdDevice = 0x1900 : `#FT_DEVICE_4222`
  bvdDevice = 0x1700 : `#FT_DEVICE_4222`
FT_DSR - Static variable in class com.ftdi.j2xx.D2xxManager
  Modem status bits :
  CTS: `D2xxManager.FT_CTS`,
  DSR: `D2xxManager.FT_DSR`,
  RI: `D2xxManager.FT_RI`,
  DCD: `D2xxManager.FT_DCD`
FT_EEPROM - Class in com.ftdi.j2xx
  EEPROM data structure on the 232A, 232B
FT_EEPROM() - Constructor for class com.ftdi.j2xx.FT_EEPROM
FT_EEPROM_2232D - Class in com.ftdi.j2xx
  EEPROM data structure on the 2232D
FT_EEPROM_2232D() - Constructor for class com.ftdi.j2xx.FT_EEPROM_2232D
FT_EEPROM_2232H - Class in com.ftdi.j2xx
  EEPROM data structure on the 2232H
FT_EEPROM_2232H() - Constructor for class com.ftdi.j2xx.FT_EEPROM_2232H
FT_EEPROM_2232H.DRIVE_STRENGTH - Class in com.ftdi.j2xx
  The driver strength on the 2232H
FT_EEPROM_2232H.DRIVE_STRENGTH() - Constructor for class com.ftdi.j2xx.FT_EEPROM_2232H.DRIVE_STRENGTH
FT_EEPROM_232H - Class in com.ftdi.j2xx
  EEPROM data structure on the 232H
FT_EEPROM_232H() - Constructor for class com.ftdi.j2xx.FT_EEPROM_232H
FT_EEPROM_232H.CBUS - Class in com.ftdi.j2xx
  CBus Option on the FT232H
FT_EEPROM_232H.CBUS() - Constructor for class com.ftdi.j2xx.FT_EEPROM_232H.CBUS
FT_EEPROM_232H.DRIVE_STRENGTH - Class in com.ftdi.j2xx
  The driver strength on the 232H
FT_EEPROM_232H.DRIVE_STRENGTH() - Constructor for class com.ftdi.j2xx.FT_EEPROM_232H.DRIVE_STRENGTH
FT_EEPROM_232R - Class in com.ftdi.j2xx
  EEPROM data structure on the 232R
FT_EEPROM_232R() - Constructor for class com.ftdi.j2xx.FT_EEPROM_232R
FT_EEPROM_232R.CBUS - Class in com.ftdi.j2xx
  CBus Option on the FT232R
FT_EEPROM_232R.CBUS() - Constructor for class com.ftdi.j2xx.FT_EEPROM_232R.CBUS
FT_EEPROM_245R - Class in com.ftdi.j2xx
  EEPROM data structure on the 245R
FT_EEPROM_245R() - Constructor for class com.ftdi.j2xx.FT_EEPROM_245R
FT_EEPROM_245R.CBUS - Class in com.ftdi.j2xx
  CBus Option on the FT245H
FT_EEPROM_245R.CBUS() - Constructor for class com.ftdi.j2xx.FT_EEPROM_245R.CBUS
FT_EEPROM_4232H - Class in com.ftdi.j2xx
  EEPROM data structure on the 4232H
FT_EEPROM_4232H() - Constructor for class com.ftdi.j2xx.FT_EEPROM_4232H
FT_EEPROM_4232H.DRIVE_STRENGTH - Class in com.ftdi.j2xx
  The driver strength on the FT4232H
FT_EEPROM_4232H.DRIVE_STRENGTH() - Constructor for class com.ftdi.j2xx.FT_EEPROM_4232H.DRIVE_STRENGTH
FT_EEPROM_X_Series - Class in com.ftdi.j2xx
  EEPROM data structure on the X Series
FT_EEPROM_X_Series() - Constructor for class com.ftdi.j2xx.FT_EEPROM_X_Series
FT_EEPROM_X_Series.CBUS - Class in com.ftdi.j2xx
  CBus Option on the X Series
FT_EEPROM_X_Series.CBUS() - Constructor for class com.ftdi.j2xx.FT_EEPROM_X_Series.CBUS
FT_EEPROM_X_Series.DRIVE_STRENGTH - Class in com.ftdi.j2xx
  The driver strength on the X Series
FT_EEPROM_X_Series.DRIVE_STRENGTH() - Constructor for class com.ftdi.j2xx.FT_EEPROM_X_Series.DRIVE_STRENGTH
FT_EVENT_LINE_STATUS - Static variable in class com.ftdi.j2xx.D2xxManager
  Event bits :
  Rx Char Event: `D2xxManager.FT_EVENT_RXCHAR`,
  Modem Status Event: `D2xxManager.FT_EVENT_MODEM_STATUS`,
  Line Status Event: `D2xxManager.FT_EVENT_LINE_STATUS`,
  Removed Event: `D2xxManager.FT_EVENT_REMOVED`
FT_EVENT_MODEM_STATUS - Static variable in class com.ftdi.j2xx.D2xxManager
  Event bits :
  Rx Char Event: `D2xxManager.FT_EVENT_RXCHAR`,
  Modem Status Event: `D2xxManager.FT_EVENT_MODEM_STATUS`,
  Line Status Event: `D2xxManager.FT_EVENT_LINE_STATUS`,
  Removed Event: `D2xxManager.FT_EVENT_REMOVED`
FT_EVENT_REMOVED - Static variable in class com.ftdi.j2xx.D2xxManager
  Event bits :
  Rx Char Event: `D2xxManager.FT_EVENT_RXCHAR`,
  Modem Status Event: `D2xxManager.FT_EVENT_MODEM_STATUS`,
  Line Status Event: `D2xxManager.FT_EVENT_LINE_STATUS`,
  Removed Event: `D2xxManager.FT_EVENT_REMOVED`
FT_EVENT_RXCHAR - Static variable in class com.ftdi.j2xx.D2xxManager
  Event bits :
  Rx Char Event: `D2xxManager.FT_EVENT_RXCHAR`,
  Modem Status Event: `D2xxManager.FT_EVENT_MODEM_STATUS`,
  Line Status Event: `D2xxManager.FT_EVENT_LINE_STATUS`,
  Removed Event: `D2xxManager.FT_EVENT_REMOVED`
FT_FE - Static variable in class com.ftdi.j2xx.D2xxManager
  Line status bits :
  OE: `D2xxManager.FT_OE`,
  PE: `D2xxManager.FT_PE`,
  FE: `D2xxManager.FT_FE`,
  BI: `D2xxManager.FT_BI`
FT_FLAGS_HI_SPEED - Static variable in class com.ftdi.j2xx.D2xxManager
  Device info list flags :
  Device Open Flag: `D2xxManager.FT_FLAGS_OPENED`,
  Device Hi Speed Flag: `D2xxManager.FT_FLAGS_HI_SPEED`
FT_FLAGS_OPENED - Static variable in class com.ftdi.j2xx.D2xxManager
  Device info list flags :
  Device Open Flag: `D2xxManager.FT_FLAGS_OPENED`,
  Device Hi Speed Flag: `D2xxManager.FT_FLAGS_HI_SPEED`
FT_FLOW_DTR_DSR - Static variable in class com.ftdi.j2xx.D2xxManager
  Flow Control bits :
  None: `D2xxManager.FT_FLOW_NONE`,
  CTS/RTS: `D2xxManager.FT_FLOW_RTS_CTS`,
  DTR/DSR: `D2xxManager.FT_FLOW_DTR_DSR`,
  XON/XOFF: `D2xxManager.FT_FLOW_XON_XOFF`
FT_FLOW_NONE - Static variable in class com.ftdi.j2xx.D2xxManager
  Flow Control bits :
  None: `D2xxManager.FT_FLOW_NONE`,
  CTS/RTS: `D2xxManager.FT_FLOW_RTS_CTS`,
  DTR/DSR: `D2xxManager.FT_FLOW_DTR_DSR`,
  XON/XOFF: `D2xxManager.FT_FLOW_XON_XOFF`
FT_FLOW_RTS_CTS - Static variable in class com.ftdi.j2xx.D2xxManager
  Flow Control bits :
  None: `D2xxManager.FT_FLOW_NONE`,
  CTS/RTS: `D2xxManager.FT_FLOW_RTS_CTS`,
  DTR/DSR: `D2xxManager.FT_FLOW_DTR_DSR`,
  XON/XOFF: `D2xxManager.FT_FLOW_XON_XOFF`
FT_FLOW_XON_XOFF - Static variable in class com.ftdi.j2xx.D2xxManager
  Flow Control bits :
  None: `D2xxManager.FT_FLOW_NONE`,
  CTS/RTS: `D2xxManager.FT_FLOW_RTS_CTS`,
  DTR/DSR: `D2xxManager.FT_FLOW_DTR_DSR`,
  XON/XOFF: `D2xxManager.FT_FLOW_XON_XOFF`
FT_OE - Static variable in class com.ftdi.j2xx.D2xxManager
  Line status bits :
  OE: `D2xxManager.FT_OE`,
  PE: `D2xxManager.FT_PE`,
  FE: `D2xxManager.FT_FE`,
  BI: `D2xxManager.FT_BI`
FT_PARITY_EVEN - Static variable in class com.ftdi.j2xx.D2xxManager
  Parity bits, used by App :
  None: `D2xxManager.FT_PARITY_NONE`,
  Odd: `D2xxManager.FT_PARITY_ODD`,
  Even: `D2xxManager.FT_PARITY_EVEN`,
  Mark: `D2xxManager.FT_PARITY_MARK`,
  Space: `D2xxManager.FT_PARITY_SPACE`
FT_PARITY_MARK - Static variable in class com.ftdi.j2xx.D2xxManager
  Parity bits, used by App :
  None: `D2xxManager.FT_PARITY_NONE`,
  Odd: `D2xxManager.FT_PARITY_ODD`,
  Even: `D2xxManager.FT_PARITY_EVEN`,
  Mark: `D2xxManager.FT_PARITY_MARK`,
  Space: `D2xxManager.FT_PARITY_SPACE`
FT_PARITY_NONE - Static variable in class com.ftdi.j2xx.D2xxManager
  Parity bits, used by App :
  None: `D2xxManager.FT_PARITY_NONE`,
  Odd: `D2xxManager.FT_PARITY_ODD`,
  Even: `D2xxManager.FT_PARITY_EVEN`,
  Mark: `D2xxManager.FT_PARITY_MARK`,
  Space: `D2xxManager.FT_PARITY_SPACE`
FT_PARITY_ODD - Static variable in class com.ftdi.j2xx.D2xxManager
  Parity bits, used by App :
  None: `D2xxManager.FT_PARITY_NONE`,
  Odd: `D2xxManager.FT_PARITY_ODD`,
  Even: `D2xxManager.FT_PARITY_EVEN`,
  Mark: `D2xxManager.FT_PARITY_MARK`,
  Space: `D2xxManager.FT_PARITY_SPACE`
FT_PARITY_SPACE - Static variable in class com.ftdi.j2xx.D2xxManager
  Parity bits, used by App :
  None: `D2xxManager.FT_PARITY_NONE`,
  Odd: `D2xxManager.FT_PARITY_ODD`,
  Even: `D2xxManager.FT_PARITY_EVEN`,
  Mark: `D2xxManager.FT_PARITY_MARK`,
  Space: `D2xxManager.FT_PARITY_SPACE`
FT_PE - Static variable in class com.ftdi.j2xx.D2xxManager
  Line status bits :
  OE: `D2xxManager.FT_OE`,
  PE: `D2xxManager.FT_PE`,
  FE: `D2xxManager.FT_FE`,
  BI: `D2xxManager.FT_BI`
FT_PURGE_RX - Static variable in class com.ftdi.j2xx.D2xxManager
  Purge flags :
  RX purge flag: `D2xxManager.FT_PURGE_RX`,
  TX purge flag: `D2xxManager.FT_PURGE_TX`
FT_PURGE_TX - Static variable in class com.ftdi.j2xx.D2xxManager
  Purge flags :
  RX purge flag: `D2xxManager.FT_PURGE_RX`,
  TX purge flag: `D2xxManager.FT_PURGE_TX`
FT_RI - Static variable in class com.ftdi.j2xx.D2xxManager
  Modem status bits :
  CTS: `D2xxManager.FT_CTS`,
  DSR: `D2xxManager.FT_DSR`,
  RI: `D2xxManager.FT_RI`,
  DCD: `D2xxManager.FT_DCD`
FT_Spi_Slave - Class in com.ftdi.j2xx.protocol
  FT SPI Slave Protocol
FT_Spi_Slave(SpiSlave) - Constructor for class com.ftdi.j2xx.protocol.FT_Spi_Slave
  FT SPI Slave Protocol Constructor
FT_STOP_BITS_1 - Static variable in class com.ftdi.j2xx.D2xxManager
  Stop bits :
  1: `D2xxManager.FT_STOP_BITS_1`,
  2: `D2xxManager.FT_STOP_BITS_2`,
FT_STOP_BITS_2 - Static variable in class com.ftdi.j2xx.D2xxManager
  Stop bits :
  1: `D2xxManager.FT_STOP_BITS_1`,
  2: `D2xxManager.FT_STOP_BITS_2`,
FTDI_BREAK_OFF - Static variable in class com.ftdi.j2xx.D2xxManager
  BREAK on is bit 14 in wValue parameter of FTDI_SET_DATA request :
  UART break on condition: `D2xxManager.FTDI_BREAK_OFF`,
  UART break off condition: `D2xxManager.FTDI_BREAK_ON`
FTDI_BREAK_ON - Static variable in class com.ftdi.j2xx.D2xxManager
  BREAK on is bit 14 in wValue parameter of FTDI_SET_DATA request :
  UART break on condition: `D2xxManager.FTDI_BREAK_OFF`,
  UART break off condition: `D2xxManager.FTDI_BREAK_ON`

A B C D E F G H I L M N O P R S T U V W

About FTDI | FTDI Licence Terms